4e6

         8
         30e3
         150
        Note: "microas" can be written "µas" in UTF-8 locales. We use the
        ASCII version here as automated systems are not always configured
        with a UTF-8 locales by default.
         90
        "degree" can be written "°" in UTF-8 locales.
         0
         0
         32

12
0 0 0
0
0.001
0
0.01
1e0
0.
Intensity
One can also specify a unit (if Gyoto was compiled with --with-udunits): Intensity[mJy/pix²] Intensity[mJy/µas²] Intensity[J.m-2.s-1.sr-1.Hz-1] Intensity[erg.cm-2.s-1.sr-1.Hz-1] Intensity[mJy.sr-1] Intensity[Jy.sr-1] The subscript "²" requires a UTF-8 locale. A normal "2" can be used instead.

12