# Converting legacy INLA mesh code to fmesher

## Deprecation warnings

Three `INLA::inla.getOption()`/`INLA::inla.setOption()` options control the transition behaviour of the `INLA` package use of `fmesher`.

- `fmesher.evolution`, integer:

  - `1L` uses the intermediate `fm_*` methods in `fmesher` that were already available via inlabru from 2.8.0, but calls the `INLA` built-in `fmesher` standalone programme for mesh construction and related operations. (From `INLA` version 23.06.29)
  - `2L` uses the full range of `fmesher` package methods, and does not use the standalone `fmesher` programme. (From `INLA` around version 23.08.20)

- `fmesher.evolution.warn`, logical: When `TRUE`, `INLA` will show deprecation methods for all the methods in `INLA` that are being replaced by `fmesher` package methods. When `FALSE`, no warnings will be shown. Set this option to `TRUE` if you want to update your own code, but keep it at `FALSE` when you need to run existing code without changing it.

- `fmesher.evolution.verbosity`, character: Either “soft”, “warn”, or “stop”, indicating the minimum warning level when `fmesher.evolution.warn` is `TRUE`. Set this to “warn” or “stop” to get more immediate feedback when testing conversion of old code, e.g. in package testing.

### Compatibility

Great effort has been taken to preserve backwards compatibility as far as practical, with in particular the old `inla.mesh`, `inla.mesh.1d`, and `inla.mesh.segment` object classes given fallback methods that carry out methods for the new `fm_mesh_2d`, `fm_mesh_1d`, and `fm_segm` classes.

An important change is that the handling of mesh `crs` information is now more flexible, but stricter in the sense that user code should make no assumption about how the information is stored in the mesh, and should therefore avoid the direct `mesh$crs` access, and instead use the `fm_crs()` and `fm_CRS()` access methods, depending on what type of CRS object is needed. The ideal way to specify crs information is in the initial mesh creation call. If the crs needs to be explicitly assigned a new value, use the `fm_crs(mesh) <- crs` assignment method.

For mesh and curve creation, the `fm_rcdt_2d_inla()`, `fm_mesh_2d_inla()`, and `fm_nonconvex_hull_inla()` methods will keep the interface syntax used by `inla.mesh.create()`, `inla.mesh.2d()`, and `inla.nonconvex.hull()` functions, respectively, whereas the `fm_rcdt_2d()`, `fm_mesh_2d()`, and `fm_nonconvex_hull()` interfaces may change in the future.

## Mesh construction

INLA | fmesher
--- | ---
`inla.mesh.create()` | `fm_rcdt_2d()` , `fm_rcdt_2d_inla()`
`inla.mesh.2d()` | `fm_mesh_2d()` , `fm_mesh_2d_inla()`
`inla.delaunay()` | `fm_delaunay_2d()`
`inla.mesh.1d()` | `fm_mesh_1d()`
`inla.mesh.lattice()` | `fm_lattice_2d()`
`inla.mesh.segment()` | `fm_segm()`
`inla.nonconvex.hull()` | `fm_nonconvex_hull()`, `fm_extensions()` , `fm_simplify()`
`inla.nonconvex.hull()` , `inla.contour.segment()`, `inla.simplify.curve()` | `fm_nonconvex_hull_inla()`, `fm_simplify_helper()` , `fm_segm_contour_helper()`

## Basis and function evaluation

INLA | fmesher
--- | ---
`inla.mesh.projector()` | `fm_evaluator()`
`inla.mesh.project()` | `fm_evaluate()`
`inla.spde.make.A()` | `fm_basis()` , `fm_row_kron()` , `inlabru::bru_mapper_multi()` , `inlabru::ibm_jacobian()` , `fm_block()` , `fm_block_eval()` , `inlabru::bru_mapper_aggregate()`
`inla.mesh.deriv()` | `fm_basis()`

## Finite element methods

INLA | fmesher | Comment
--- | --- | ---
`inla.mesh.fem()` , `inla.mesh.1d.fem()` | `fm_fem()` |
`` | `fm_matern_precision()` |
`` | `fm_matern_sample()` | Convenience function that combines `fm_matern_precision()` and `fm_sample()`.
`` | `fm_covariance()` | Basic helper function for computing covariances between different locations. Can produce sparse inverses like `inla.qinv()`, but currently (version 0.1.1) only by a ‘brute force’ method.
`` | `fm_sample()` | Basic sampling method, like `inla.qsample()`

## Printing

INLA | fmesher | Comments
--- | --- | ---
`summary.inla.mesh()` | `print.fm_mesh_2d()`, `print.fm_segm()` , `print.fm_mesh_1d()` | Use `print(mesh)` etc.

## CRS information and coordinate transformations

INLA | fmesher | Comments
--- | --- | ---
`inla.spTransform()` | `fm_transform()` |
`mesh$crs` | `fm_crs(mesh)` , `fm_CRS(mesh)` | The crs may now be stored in different formats; use `fm_crs()` for `sf` format, and `fm_CRS()` for `sp` format. `fmesher` will attempt to convert when needed.
`mesh$crs<-` | `fm_crs(mesh)<-` | Direct assignment of crs information should be avoided, but is allowed as long as its compatible with the actual mesh coordinates.

## Plotting

INLA | fmesher | Comment
--- | --- | ---
`No ggplot support` | `geom_fm(data = mesh)`, `geom_fm(data = segm)` | Use `ggplot() + geom_fm(data = mesh)` and `inlabru::gg()` methods
`plot.inla.mesh(rgl = FALSE)` | `plot.fm_mesh_2d()` , `lines.fm_mesh_2d()` | Use `plot()` or `lines()`
`lines.inla.mesh.segment(rgl = FALSE)` | `plot.fm_segm()` , `lines.fm_segm()` | Use `plot()` or `lines()`
`plot.inla.mesh(rgl = TRUE)` | `plot_rgl()` , `lines_rgl()` |
`lines.inla.mesh.segment(rgl = TRUE)` | `plot_rgl()` , `lines_rgl()` |